; stop.g
; called when M0 (Stop) is run (e.g. when a print from SD card is cancelled)
;
; generated by RepRapFirmware Configuration Tool v3.2.3 on Wed May 26 2021 19:44:39 GMT+0000 (Coordinated Universal Time)

