; homey.g
; called to home the Y axis
;
M201 X500.00 Y500.00    ; Reduce acceleration for homing moves
G91               ; relative positioning
G1 H2 Z10 F8000   ; lift Z relative to current position
G1 H1 Y625 F3600  ; move quickly to Y axis endstop and stop there (first pass)
G1 Y-20 F3000     ; go back a few mm
G1 H1 Y625 F256   ; move slowly to Y axis endstop once more (second pass)
G1 Y10 F10800     ; move forward 10 mm
M201 X3000 Y3000  ; Return to full accelerationG1 H2 Z-10 F10800
G1 H2 Z-10 F8000  ; Lower Z relative to current position
G90               ; absolute positioning

