; 0:/macros/PID Tuning/PID Tune Hot End 220
; Based on https://duet3d.dozuki.com/Wiki/Tuning_the_heater_temperature_control
;

M291 S3 R"PID Tuning Bed to 110c" P"Do not interrupt or leave unattended while tuning in progress."

M303 H0 S110 		; auto tune heater 0, default PWM, 60C target or maximum temperature

M98 P"0:/macros/Musical Tunes/TwoBits.g"

M291 S3 R"PID Tuning Complete" P"Check console for heater values. Values saved to config-Override.g"

M307 H1			; report values for heater 1
M500			; Save values to config-override.g
